A picture containing text, clock, table

Description automatically generated

Version: S350H\_SLDR\_HUNG\_Tech\_Doc\_021222\_Vev1

**SERIES 350 Hybrid**

Horizontal Slider and

Vertical Single Hung

Windows

Technical Specifications

and Cross-Sectional

Details

**Table of Contents**

[CONSTRUCTIONS SPECIFICATIONS - SECTION 08 54 00 3](#_Toc95581010)

[PART 1 GENERAL 3](#_Toc95581011)

[1.1. SECTION INCLUDES 3](#_Toc95581012)

[1.2. REFERENCES 3](#_Toc95581013)

[1.3. SUBMITTALS 4](#_Toc95581014)

[1.4. QUALITY ASSURANCE 4](#_Toc95581015)

[1.5. STORAGE AND HANDLING 4](#_Toc95581016)

[1.6. WARRANTY 4](#_Toc95581017)

[PART 2 PRODUCTS 4](#_Toc95581018)

[2.1. MANUFACTURED UNITS 4](#_Toc95581024)

[2.2. FRAME DESCRIPTION 5](#_Toc95581025)

[2.3. WEATHER STRIP 6](#_Toc95581026)

[2.4. JAMB EXTENSION 6](#_Toc95581027)

[2.5. INSECT SCREEN 6](#_Toc95581028)

[2.6. GRILLES-BETWEEN-THE–GLASS 6](#_Toc95581029)

[2.7. SIMULATED DIVIDED LITES (SDL) 6](#_Toc95581030)

[2.8. ACCESSORIES AND TRIM 6](#_Toc95581031)

[PART 3 EXECUTION 7](#_Toc95581032)

[3.1. EXAMINATION 7](#_Toc95581037)

[3.2. INSTALLATION 7](#_Toc95581038)

[3.3. FIELD QUALITY CONTROL 7](#_Toc95581039)

[3.4. CLEANING 7](#_Toc95581040)

[3.5. PROTECTING INSTALLED CONSTRUCTION 7](#_Toc95581041)

[WINDOW TYPE AND CLASSIFICATIONS 8](#_Toc95581042)

[ENERGY STAR 9](#_Toc95581043)

[THERMAL RESULTS 11](#_Toc95581044)

[HORIZONTAL SLIDER WINDOW 11](#_Toc95581045)

[VERTICAL SINGLE HUNG WINDOW 12](#_Toc95581046)

[CROSS SECTION DETAILS 13](#_Toc95581047)

[HORIZONTAL SLIDER WINDOW 13](#_Toc95581048)

[VERTICAL SINGLE HUNG WINDOW 14](#_Toc95581049)

[MULLING ASSEMBLY – HORIZONTAL SLIDER 15](#_Toc95581050)

[MULLING ASSEMBLY – VERTICAL SINGLE HUNG 16](#_Toc95581051)

[GRILL + SDL OPTIONS 17](#_Toc95581052)

[TEST REPORTS 18](#_Toc95581053)

# CONSTRUCTIONS SPECIFICATIONS - SECTION 08 54 00

# PART 1 GENERAL

## SECTION INCLUDES

1. Series 350 Hybrid Horizontal Slider Window complete with hardware, glazing, mulling options, weather strip, insect screen, grilles-between-the-glass, jamb extension, exterior brickmould trims, exterior sill extension and standard or specified anchors, trim and attachments
2. Series 350 Hybrid Vertical Single Hung Window complete with hardware, glazing, mulling options, weather strip, insect screen, grilles-between-the-glass, jamb extension, exterior brickmould trims, exterior sill extension and standard or specified anchors, trim and attachments

## REFERENCES

1. ASTM International (ASTM):
   * + 1. American Society for Testing and Materials (ASTM):
2. C1036: Standard Specification for Flat Glass.
3. E 283: Standard Test Method for Rate of Air Leakage through Exterior Windows, Curtain Walls and Doors.
4. E 330: Standard Test Method for Structural Performance of Exterior Windows, Curtain Walls, and Door by Uniform Static Air Pressure Difference.
5. E 547: Standard Test Method for Water Penetration of Exterior Windows, Curtain Walls, and Doors by Cyclic Static Air Pressure Differential.
6. E 2190: Standard Specification for Insulating Glass Unit Performance Evaluation.
7. F 2090-10: Standard Specification for Window Fall Prevention Devices with Emergency Escape (Egress) Release Mechanisms.
8. American Architectural Manufacturer’s Association/Window and Door Manufacturer’s Association/Canadian Standards Association (AAMA/WDMA/CSA): (use appropriate specifications depending on certification for each product type).
9. AAMA/WDMA/CSA 101/I.S.2/A440-08/11,S11-09, S1-17: North American Fenestration Standard/Specification for windows, doors, and skylights.
10. AAMA 450-10: Voluntary Performance Rating Method for Mulled Fenestration Assemblies
11. Window and Door Manufacturer’s Association (WDMA): Keystone Certification Program
12. Insulating Glass Manufacturer’s Alliance/Insulating Glass Certification Council (IGMA/IGCC).
13. National Fenestration Rating Council (NFRC):
14. 101: Procedures for Determining Fenestration Product Thermal Properties.
15. 200: Procedure for Determining Solar Heat Gain Coefficients at Normal Incidence

## SUBMITTALS

1. Shop Drawings: Submit shop drawings.
2. Samples: Specified performance and design requirements.
3. Quality Control Submittals: Certificates: Submit manufacturer’s certification indicating compliance with specified performance and design requirement

## QUALITY ASSURANCE

1. Requirements: consult local code for NBC [National Building Code] adoption year and pertinent revisions for information on:
2. Egress, emergency escape and rescue requirements.
3. Basement window requirements.
4. Windows fall prevention and/or window opening control device requirements.

## STORAGE AND HANDLING

1. Applicable frames and mulled units will include additional bracing to maintain squareness and rigidity during shipment.
2. Store window units in an upright position in a clean and dry storage area above ground to protect from weather.

## WARRANTY

**The following limited warranty is subject to conditions and exclusions. There are certain conditions or applications over which EVERLAST Group of Companies has no control. Defect or problems as a result of such conditions or applications are not the responsibility of EVERLAST Groups of Companies. For a more complete description of the EVERLAST limited warranty, refer to the complete and current warranty information available by request.**

Clear insulating glass with stainless steel spacers is warranted against seal failure caused by manufacturing defects and resulting in visible obstruction through the glass for twenty (20) years from the original date of purchase. Glass is warranted against stress cracks caused by manufacturing defects from ten (10) years from the original date of purchase.

Hardware and other non-glass components are warranted to be free from manufacturing defects for two (2) years from the original date of purchase.

# PART 2 PRODUCTS



## MANUFACTURED UNITS

1. Description: Altitude Casement / Awning units as manufactured by EVERLAST Group of Companies
   * Calgary, Alberta, Canada

## FRAME DESCRIPTION

1. Frame:
2. Frame – Vinyl: Members shall be manufactured from 0.079” [2mm] extruded unplasticized polyvinylchloride (uPVC). Frame corners shall be fusion welded and cleaned.
3. Frame Depth – Vinyl: Frame shall have standard jamb depth of 3-1/4” [83mm] with integral nailing fin and an overall profile thickness of 4-1/4” [108mm].
4. Frame Exterior Cladding: Manufactured from 0.070” [2mm] extruded aluminum.
5. Interior and exterior frame expander accessory are factory installed.
6. Interior and exterior fabricated frame expander components, including head-jamb, sill and both jamb components.
7. SASH DESCRIPTION
8. Sash: Unplasticized polyvinylchloride (uPVC). Sash corners shall be fusion welded and cleaned.
9. Sash Profile: Shall be 2-3/16” [55mm] in thickness
10. Sash Exterior Cladding: Manufactured from 0.070” [2mm] extruded aluminum.
11. GLAZING
12. Select quality complying with ASTM C 1036. Insulating glass SIGMA/IGCC when tested in accordance with ASTM E 2190. STC/OITC ratings are tested to the stated performance level in accordance with ASTM E 90-09.
13. Glazing Method: 1 3/16” (30mm) insulating glass. Dual and Triple glazing.
14. Glass Type: LoE Cardinal IG® i89,180, 270, 272 and 366 with Air or Argon Gas.
15. Glass Type Options: Obscure Glass, Sand Blasted, Rain Glass, Glue Chip, Narrow Reed, Reed, Bronze Tint, Gray Tint, Green Tint.
16. Glazing Seal: Pressure gasket at exterior; interior has glazing boot inserted.
17. Perimeter Spacer: Default color is mill finish (stainless).
18. Glazing Option: STC/OITC upgrade.
19. MULLING
20. Directional mull limits: 6 wide by 1 unit high; Rough Opening not to exceed 114” x 84” (2896mm x 2134mm).
21. Directional mull limits: 5 units wide by 5 units high: Rough Opening not to exceed 96” x 84” (2438mm x 2134mm).
22. FINISH
23. Exterior Vinyl Colour: Standard white.
24. Exterior Cladding Colour: Matte Black, White, Slate Grey and Commercial Brown. Custom colour available upon request to a Everlast representative,
25. HARDWARE
26. Lock: Zinc die-cast sash lock and keeper. Two locks are applied to all units with 30” [762mm] rough opening width and wider
27. Single Hung Balances: Inverted, constant-force stainless steel coil system contained in pivot, locking shoe, housed in a rigid vinyl jamb liner. Balance system must meet AAMA 902-07 Class 3 requirements. Zinc die-cast sash pins disengage sash for easy removal
28. Horizontal Slider Rollers: Acetal non-marking roller sets.
29. Colour: Applies to handle and locking hardware:
30. Standard Color: Matte Black and White; other colours are also available.

## WEATHER STRIP

1. Woven pile weather stripping with mylar fin applied around full perimeter of operating sash and frame.
2. Standard weather strip color: white, tri-fin.

## JAMB EXTENSION

1. Standard: factory-installed jamb extension; various sizes and finishes available.

## INSECT SCREEN

1. Tested to ASTM E-1748-95(09).
2. Factory-installed screen; screen mesh: charcoal fiberglass.
3. Aluminum frame finish: Matches interior colour options.

## GRILLES-BETWEEN-THE–GLASS

1. Manufactured from aluminum profile placed between the two panes of glass.
2. Interior Colours: Various colours, including split finishes are available.
3. Exterior Colours: Various colours, including split finishes are available.
4. Profiles: Various profile shapes are available, contact an Everlast representative.
5. Pattern: Various patterns are available, contact an Everlast representative. .

## SIMULATED DIVIDED LITES (SDL)

1. Size: 1” (25mm) wide, 2” (50mm) wide with or w/out internal spacer bar; w/out is standard.
2. Colours: Various standard and custom colours available, contact an EVERLAST representative.

## ACCESSORIES AND TRIM

1. Exterior Casing: Offset brickmould available in standard and custom colors.
2. Installation Accessories: Factory-installed aluminum nailing fin at head, sill and side jambs.
3. Installation brackets
4. Mullion kit: standard mullion kit for filed assembly of related units available. Kit includes: Instruction, interior and exterior mull covers and brackets.

# PART 3 EXECUTION



## EXAMINATION

1. Verification of Condition: Before installation, verify openings are plumb, square and of proper dimensions. Report frame defects or unsuitable conditions to the General Contractor and/or Everlast directly before proceeding. Damages or defects must be reported within 72 hours of receipt of finished goods.
2. Acceptance of Condition: Beginning installation or no notification within the 72 hours confirms acceptance of existing conditions.

## INSTALLATION

1. Assemble and install window/door unit(s) according to manufacturer’s instruction and reviewed shop drawing.
2. Install sealant and related backing materials at perimeter of unit or assembly in accordance to reviewed shop drawings.
3. Install accessory items as required.

## FIELD QUALITY CONTROL

1. Remove visible labels and adhesive residue according to manufacturers’ instruction
2. Unless otherwise specified, water penetration resistance testing shall be conducted per AAMA 502 and ASTM E1105 at 2/3 of the fenestration products design pressure (DP) rating. Water penetration shall be defined in accordance with the test method(s) applied.

## CLEANING

1. Remove visible labels and adhesive residue according to manufacturer’s instruction.
2. Leave windows and glass in a clean condition.

## PROTECTING INSTALLED CONSTRUCTION

1. Protecting windows from damage by chemicals, solvents, paint or other construction operations that may cause damage.

**END OF SECTION**

# WINDOW TYPE AND CLASSIFICATIONS

Design Performance Classifications

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Product** | **Air**  **Tested**  **psf** | **Water**  **Tested  Pa** | **Design**  **Pressure**  **(Uniform Load)**  **Pa / psf** | | **Cert. Rating** | **Test Size** | | | |
| **Max  Overall Width** | | **Max  Overall Height** | |
| **in** | **mm** | **in** | **mm** |
| Horizontal Slider | A3 | 360 | 2160/  -2160 | 45.11 | LC-  PG45 | 70 7/8” | 1800 | 55 1/8” | 1400 |
| Vertical Single Hung | A3 | 470 | 3120/  -3120 | 65.16 | LC-  PG65 | 43 | 1100 | 75” | 1900 |

Screen Testing Performance

|  |  |  |
| --- | --- | --- |
| **Product** | **Canadian Supplement**  **A440-S01-09** | |
| Horizontal Slider | ASTM E1748-95(09) | Passed |
| Vertical Single Hing | ASTM E1748-95(09 | Passed |

# ENERGY STAR

ENERGY STAR® Program - Canada

This technical specification determines how residential windows, doors, and skylights sold in Canada are certified for the ENERGY

STAR® program. This specification is issued by Natural Resources Canada (NRCan). NRCan has been authorized by the U.S. Environmental Protection Agency (EPA) to promote and administer the ENERGY STAR name and symbol in Canada. A product must meet this specification in order to be promoted as ENERGY STAR certified in Canada by its manufacturer or authorized agent. Manufacturers must also sign a Fenestration Administrative Arrangement with NRCan.

Performance metrics

U-Factor: The heat transfer per time per area and per degree of temperature difference in W/m2∙K (Btu/h ft2∙˚F). The U-factor multiplied by the interior-exterior temperature difference and by the projected fenestration product area yields the total heat transfer

through the fenestration product due to conduction, convection, and long-wave infra-red radiation. A U-factor in Btu/h ft2·°F multiplied by 5.678263 converts the value to W/m2·K. The U-factor in Btu/h ft2·°F shall conform with Table 1 before the conversion to W/m2·K.

Solar heat gain coefficient (SHGC): The ratio of the solar heat gain entering the space through the fenestration product to the incident solar radiation.

Air leakage: the flow of air that passes through fenestration products in L/s/m2. Air leakage infiltration is the flow of air into the building envelope and exfiltration is the flow of air out of the building envelope. An air leakage in cfm/ft2 multiplied by 5.08 converts the value to L/s/m2. The air leakage value in cfm/ft2 shall conform with Table 1 before the conversion to L/s/m2.

Energy rating (ER): a unitless value derived from a formula that balances heat loss (U-factor), air leakage loss and potential passive solar gain of a fenestration product. The ER is applied to fenestration systems intended to be installed in a vertical orientation in low-rise residential buildings. The simplified ER equation is as follows:

ER = (57.76 × SHGCw) – (21.90 × Uw) – (1.97 × L75) + 40 where

* SHGCw = fenestration system solar heat gain coefficient
* Uw = fenestration system U-factor (W/m2)
* L75 = fenestration system air leakage rate at a pressure difference of 75 Pa, established in accordance with AAMA/WDMA/CSA 101/I.S.2/A440 (North American Fenestration Standard) in L/s•m2. The L75 shall be the average of the infiltration and exfiltration measurements.

A complete explanation of the ER equation may be found in the CSA A440.2 Standard.

U-factor Criteria for Residential Windows and Doors

|  |  |  |
| --- | --- | --- |
| **Product** | **Maximum U-factor W/m2∙K** | **Maximum U-factor Btu/h∙ft2◦F** |
| Windows and Doors | 1.22 | 0.21 |

Alternate ER Criteria for Residential Windows and Doors

|  |  |
| --- | --- |
| **Product** | **Minimum ER (unitless)** |
| Windows and Doors | 34 |

U-factor Criteria for Unit Skylights

|  |  |  |
| --- | --- | --- |
| **Product** | **Maximum U-factor W/m2∙K** | **Maximum U-factor Btu/h∙ft2◦F** |
| Skylights | 2.29 | 0.4 |

# THERMAL RESULTS

## HORIZONTAL SLIDER WINDOW

Table

Description automatically generatedTable

Description automatically generated

## VERTICAL SINGLE HUNG WINDOW

Table

Description automatically generated

Table

Description automatically generated

# CROSS SECTION DETAILS

## HORIZONTAL SLIDER WINDOW

Diagram, schematic

Description automatically generated

## VERTICAL SINGLE HUNG WINDOW

Diagram, schematic

Description automatically generated

## MULLING ASSEMBLY – HORIZONTAL SLIDER

Diagram

Description automatically generated

## MULLING ASSEMBLY – VERTICAL SINGLE HUNG

Diagram, schematic

Description automatically generated

## GRILL + SDL OPTIONS

Diagram, schematic

Description automatically generated

# TEST REPORTS

Table

Description automatically generated

Table

Description automatically generated